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- screw L/o: a4:1

|- Screw Revolution: S54rom
|- Gear box ratio: 1:3.16
|- Barre! Biock: 11Blocks
|- orive Power: 300kw

|- Heater Capacity: 99.3kw
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